{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["LinkedGems","IndepGems","MicroMega"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"LinkedGems","index":0,"n_rows":68,"n_cols":29,"rows_kept":68,"cut":false,"hidden":false,"merged":[[45,0,45,2],[5,0,5,2],[15,0,15,2],[25,0,25,2],[35,0,35,2]],"flags":["formulas_cached_only"]}
[null,"Voltage Divider Circuit for Test Chamber with GEMs"]
[]
[]
[]
[]
["Varying the voltage across GEM2"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Veq8","Veq7","Veq6","Veq5","Veq4","Veq3","Veq2","Veq1","Veq0","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,-2780.000000000002,-3020.000000000002,-3260.000000000002,-3500.000000000002,-3740.000000000002,-3980.000000000002,-4220.000000000002,-4460.000000000002,-4700.000000000002,150,-4940.000000000002,10,0.3,1,0.6666666666666667,1,52.916666666666636,5,-48.000000000000036]
[0,2000,-350,-1000,-1350,-2000,-400,-1950,-2350,-2590,-2830.000000000001,-3070.000000000001,-3310.000000000001,-3550.000000000001,-3790.000000000001,-4030.000000000001,-4270.000000000001,-4510.000000000001,-4750.000000000001,150,-4990.000000000001,10,0.35,1,0.6666666666666667,1,53.958333333333314,5,-48.000000000000014]
[0,2000,-400,-1000,-1400,-2000,-400,-2000,-2400,-2640,-2879.999999999998,-3119.999999999998,-3359.999999999998,-3599.999999999998,-3839.999999999998,-4079.999999999998,-4319.999999999998,-4559.999999999998,-4799.999999999998,150,-5039.999999999998,10,0.4,1,0.6666666666666667,1,55.00000000000006,5,-47.99999999999996]
[0,2000,-450,-1000,-1450,-2000,-400,-2050,-2450,-2690,-2930.000000000002,-3170.000000000002,-3410.000000000002,-3650.000000000002,-3890.000000000002,-4130.000000000002,-4370.000000000002,-4610.000000000002,-4850.000000000002,150,-5090.000000000002,10,0.45,1,0.6666666666666667,1,56.04166666666663,5,-48.000000000000036]
[]
[]
[]
["Varying the voltage across GEM1"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Veq8","Veq7","Veq6","Veq5","Veq4","Veq3","Veq2","Veq1","Veq0","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,-2780.000000000002,-3020.000000000002,-3260.000000000002,-3500.000000000002,-3740.000000000002,-3980.000000000002,-4220.000000000002,-4460.000000000002,-4700.000000000002,150,-4940.000000000002,10,0.3,1,0.6666666666666667,1,52.916666666666636,5,-48.000000000000036]
[0,2000,-300,-1000,-1300,-2000,-450,-1900,-2350,-2590,-2830.000000000001,-3070.000000000001,-3310.000000000001,-3550.000000000001,-3790.000000000001,-4030.000000000001,-4270.000000000001,-4510.000000000001,-4750.000000000001,150,-4990.000000000001,10,0.3,1,0.75,1,53.958333333333314,5,-48.000000000000014]
[0,2000,-300,-1000,-1300,-2000,-500,-1900,-2400,-2640,-2879.999999999998,-3119.999999999998,-3359.999999999998,-3599.999999999998,-3839.999999999998,-4079.999999999998,-4319.999999999998,-4559.999999999998,-4799.999999999998,150,-5039.999999999998,10,0.3,1,0.8333333333333333,1,55.00000000000006,5,-47.99999999999996]
[0,2000,-300,-1000,-1300,-2000,-550,-1900,-2450,-2690,-2930.000000000002,-3170.000000000002,-3410.000000000002,-3650.000000000002,-3890.000000000002,-4130.000000000002,-4370.000000000002,-4610.000000000002,-4850.000000000002,150,-5090.000000000002,10,0.3,1,0.9166666666666667,1,56.04166666666663,5,-48.000000000000036]
[]
[]
[]
["Varying the Induction Field"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Veq8","Veq7","Veq6","Veq5","Veq4","Veq3","Veq2","Veq1","Veq0","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,1500,-300,-750,-1050,-2000,-400,-1650,-2050,-2290,-2530.000000000001,-2770.000000000001,-3010.000000000001,-3250.000000000001,-3490.000000000001,-3730.000000000001,-3970.000000000001,-4210.000000000001,-4450.000000000001,150,-4690.000000000001,10,0.4,1,0.6666666666666667,1,47.70833333333332,5,-48.00000000000002]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,-2780.000000000002,-3020.000000000002,-3260.000000000002,-3500.000000000002,-3740.000000000002,-3980.000000000002,-4220.000000000002,-4460.000000000002,-4700.000000000002,150,-4940.000000000002,10,0.3,1,0.6666666666666667,1,52.916666666666636,5,-48.000000000000036]
[0,2500,-300,-1250,-1550,-2000,-400,-2150,-2550,-2790,-3029.999999999998,-3269.999999999998,-3509.999999999998,-3749.999999999998,-3989.999999999998,-4229.999999999998,-4469.999999999998,-4709.999999999998,-4949.999999999998,150,-5189.999999999998,10,0.24,1,0.6666666666666667,1,58.12500000000006,5,-47.99999999999996]
[0,3000,-300,-1500,-1800,-2000,-400,-2400,-2800,-3040,-3280.000000000001,-3520.000000000001,-3760.000000000001,-4000.000000000001,-4240.000000000001,-4480.000000000001,-4720.000000000001,-4960.000000000001,-5200.000000000001,150,-5440.000000000001,10,0.2,1,0.6666666666666667,1,63.333333333333314,5,-48.000000000000014]
[]
[]
[]
["Varying the Transfer Field"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Veq8","Veq7","Veq6","Veq5","Veq4","Veq3","Veq2","Veq1","Veq0","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,2000,-300,-1000,-1300,-1500,-400,-1750,-2150,-2390,-2630.000000000001,-2870.000000000001,-3110.000000000001,-3350.000000000001,-3590.000000000001,-3830.000000000001,-4070.000000000001,-4310.000000000001,-4550.000000000001,150,-4790.000000000001,10,0.3,1,0.8888888888888888,1,49.79166666666664,5,-48.00000000000002]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,-2780.000000000002,-3020.000000000002,-3260.000000000002,-3500.000000000002,-3740.000000000002,-3980.000000000002,-4220.000000000002,-4460.000000000002,-4700.000000000002,150,-4940.000000000002,10,0.3,1,0.6666666666666667,1,52.916666666666636,5,-48.000000000000036]
[0,2000,-300,-1000,-1300,-2500,-400,-2050,-2450,-2690,-2930.000000000002,-3170.000000000002,-3410.000000000002,-3650.000000000002,-3890.000000000002,-4130.000000000002,-4370.000000000002,-4610.000000000002,-4850.000000000002,150,-5090.000000000002,10,0.3,1,0.5333333333333334,1,56.04166666666663,5,-48.000000000000036]
[0,2000,-300,-1000,-1300,-3000,-400,-2200,-2600,-2840,-3080.0000000000027,-3320.0000000000027,-3560.0000000000027,-3800.0000000000027,-4040.0000000000027,-4280.000000000003,-4520.000000000003,-4760.000000000003,-5000.000000000003,150,-5240.000000000003,10,0.3,1,0.4444444444444444,1,59.166666666666586,5,-48.000000000000064]
[]
[]
[]
["Varying the Drift Field"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Veq8","Veq7","Veq6","Veq5","Veq4","Veq3","Veq2","Veq1","Veq0","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,-2780.000000000002,-3020.000000000002,-3260.000000000002,-3500.000000000002,-3740.000000000002,-3980.000000000002,-4220.000000000002,-4460.000000000002,-4700.000000000002,150,-4940.000000000002,10,0.3,1,0.6666666666666667,1,52.916666666666636,5,-48.000000000000036]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2620,-2939.999999999999,-3259.999999999999,-3579.999999999999,-3899.999999999999,-4219.999999999999,-4539.999999999999,-4859.999999999999,-5179.999999999999,-5499.999999999999,200,-5819.999999999999,10,0.3,1,0.6666666666666667,1,40.93750000000001,5,-63.99999999999999]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2700,-3100,-3500,-3900,-4300,-4700,-5100,-5500,-5900,-6300,250,-6700,10,0.3,1,0.6666666666666667,1,33.75,5,-80]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2780,-3260.000000000002,-3740.000000000002,-4220.000000000002,-4700.000000000002,-5180.000000000002,-5660.000000000002,-6140.000000000002,-6620.000000000002,-7100.000000000002,300,-7580.000000000002,10,0.3,1,0.6666666666666667,1,28.958333333333325,5,-96.00000000000003]
[]
[]
[]
[null,"Extreme Conditions"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Veq8","Veq7","Veq6","Veq5","Veq4","Veq3","Veq2","Veq1","Veq0","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,4.269230769230768,1,-1040.0000000000002]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,8.538461538461537,2,-520.0000000000001]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,12.807692307692305,3,-346.66666666666674]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,17.076923076923073,4,-260.00000000000006]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,21.34615384615384,5,-208.00000000000006]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,25.61538461538461,6,-173.33333333333337]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,29.88461538461538,7,-148.57142857142858]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,34.153846153846146,8,-130.00000000000003]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,38.42307692307691,9,-115.55555555555559]
[0,3000,-450,-1500,-1950,-3000,-550,-2850,-3400,-4440,-5480.000000000002,-6520.000000000002,-7560.000000000002,-8600.000000000002,-9640.000000000002,-10680.000000000002,-11720.000000000002,-12760.000000000002,-13800.000000000002,650,-14840.000000000002,10,0.3,1,0.6111111111111112,1,42.69230769230768,10,-104.00000000000003]

{"sheet":"IndepGems","index":1,"n_rows":49,"n_cols":20,"rows_kept":49,"cut":false,"hidden":false,"merged":[[42,0,42,2],[5,0,5,2],[14,0,14,2],[23,0,23,2],[32,0,32,2]],"flags":["formulas_cached_only"]}
[null,"Voltage Divider Circuit for Test Chamber with GEMs"]
[]
[{"$nulls":6},"Purple = Voltage Setting",{"$nulls":6},"Blue = constant"]
[{"$nulls":13},"Red = variable"]
[]
["Varying the voltage across GEM2"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,150,-4940.000000000002,10,0.30927835051546393,1,0.2150537634408602,1,63.49999999999996,6,-40.00000000000003]
[0,2000,-350,-1000,-1350,-2000,-400,-1950,-2350,-2590,150,-4990.000000000001,10,0.36269430051813484,1,0.20942408376963342,1,64.74999999999997,6,-40.000000000000014]
[0,2000,-400,-1000,-1400,-2000,-400,-2000,-2400,-2640,150,-5039.999999999998,10,0.41666666666666663,1,0.20408163265306117,1,66.00000000000006,6,-39.999999999999964]
[0,2000,-450,-1000,-1450,-2000,-400,-2050,-2450,-2690,150,-5090.000000000002,10,0.4712041884816754,1,0.19900497512437806,1,67.24999999999994,6,-40.000000000000036]
[]
[]
["Varying the voltage across GEM1"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,150,-4940.000000000002,10,0.30927835051546393,1,0.2150537634408602,1,63.49999999999996,6,-40.00000000000003]
[0,2000,-300,-1000,-1300,-2000,-450,-1900,-2350,-2590,150,-4990.000000000001,10,0.30927835051546393,1,0.24258760107816718,1,64.74999999999997,6,-40.000000000000014]
[0,2000,-300,-1000,-1300,-2000,-500,-1900,-2400,-2640,150,-5039.999999999998,10,0.30927835051546393,1,0.2702702702702702,1,66.00000000000006,6,-39.999999999999964]
[0,2000,-300,-1000,-1300,-2000,-550,-1900,-2450,-2690,150,-5090.000000000002,10,0.30927835051546393,1,0.2981029810298103,1,67.24999999999994,6,-40.000000000000036]
[]
[]
["Varying the Induction Field",{"$nulls":15},"s"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,1500,-300,-750,-1050,-2000,-400,-1650,-2050,-2290,150,-4690.000000000001,10,0.41666666666666663,1,0.24844720496894407,1,57.249999999999986,6,-40.000000000000014]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,150,-4940.000000000002,10,0.30927835051546393,1,0.2150537634408602,1,63.49999999999996,6,-40.00000000000003]
[0,2500,-300,-1250,-1550,-2000,-400,-2150,-2550,-2790,150,-5189.999999999998,10,0.24590163934426226,1,0.18957345971563994,1,69.75000000000006,6,-39.99999999999997]
[0,3000,-300,-1500,-1800,-2000,-400,-2400,-2800,-3040,150,-5440.000000000001,10,0.20408163265306117,1,0.1694915254237289,1,75.99999999999997,6,-40.000000000000014]
[]
[]
["Varying the Transfer Field"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,2000,-300,-1000,-1300,-1500,-400,-1750,-2150,-2390,150,-4790.000000000001,10,0.30927835051546393,1,0.23391812865497083,1,59.74999999999997,6,-40.000000000000014]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,150,-4940.000000000002,10,0.30927835051546393,1,0.2150537634408602,1,63.49999999999996,6,-40.00000000000003]
[0,2000,-300,-1000,-1300,-2500,-400,-2050,-2450,-2690,150,-5090.000000000002,10,0.30927835051546393,1,0.19900497512437806,1,67.24999999999994,6,-40.000000000000036]
[0,2000,-300,-1000,-1300,-3000,-400,-2200,-2600,-2840,150,-5240.000000000003,10,0.30927835051546393,1,0.18518518518518523,1,70.99999999999991,6,-40.00000000000005]
[]
[]
[]
["Varying the Drift Field"]
["Anode","Induction Gap","GEM2","GEM2","GEM2","Transfer Gap","GEM1","GEM1","GEM1","Veq9","Drift Gap","Cathode","Rload","RG2","RT","RG1","RT'","RF","Req","I     (microA)"]
["(V)","(V/cm)","Differential","Bottom (V)","Top (V)","(V/cm)","Differential (V)","Bottom (V)","Top (V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","(MOhm)","across Drift Field circuit"]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2540,150,-4940.000000000002,10,0.30927835051546393,1,0.2150537634408602,1,63.49999999999996,6,-40.00000000000003]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2620,200,-5819.999999999998,10,0.30927835051546393,1,0.2150537634408602,1,49.125000000000014,6,-53.33333333333331]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2700,250,-6700,10,0.30927835051546393,1,0.2150537634408602,1,40.5,6,-66.66666666666667]
[0,2000,-300,-1000,-1300,-2000,-400,-1900,-2300,-2780,300,-7580.000000000001,10,0.30927835051546393,1,0.2150537634408602,1,34.74999999999999,6,-80.00000000000001]

{"sheet":"MicroMega","index":2,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[[6,0,6,2],[13,1,13,2],[15,0,15,2]],"flags":["formulas_cached_only"]}
[null,null,"Voltage Divider Circuit for Test Chamber with Micromega"]
[]
[]
[null,null,"Purple = Voltage Setting",null,null,null,"Blue =constant"]
[]
[]
["Varying the Induction Field"]
["Anode","Induction Gap","Micromega (V1)","Veq9","Drift Gap","Cathode","Rload","RF","Req"]
["(V)","(kV/cm)","(V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)"]
[0,40,-400,-640,150,-3040,10,0.8,0.3]
[0,45,-450,-690,150,-3277.5,10,0.8,0.3]
[0,50,-500,-740,150,-3515,10,0.8,0.3]
[0,55,-550,-790,150,-3752.5,10,0.8,0.3]
[null,"* assuming a 100micron gap"]
[]
["Varying the Drift Field"]
["Anode","Induction Gap","Micromega (V1)","Veq9","Drift Gap","Cathode","Rload","RF","Req"]
["(V)","(kV/cm)","(V)","(V)","(V/cm)","(V)","(MOhm)","(MOhm)","(MOhm)"]
[0,40,-400,-640,150,-3040,10,0.8,0.3]
[0,40,-400,-720,200,-3420,10,0.8,0.3]
[0,40,-400,-800,250,-3800,10,0.8,0.3]
[0,40,-400,-880,300,-4180,10,0.8,0.3]