Cryomodules

Info

Down in the LINAC tunnel, there are a total of 46 cryomodules in the beamline. Each one of these modules houses the cavities used to accelerate the beam. The cavities need to be supercooled to very low temperatures, so the cryomodules have cooling lines that use liquid helium to do so. The CA modules have 4 cavities each, CB have 8 each, CC have 6 each, and the CD have 8 each.

Tips and Notes

Location

LEBT

RFQ

MEBT

LS1

LS2

LS3

PV's

LS1_CA01 - LS1_CA03

LS1_CB01 - LS1_CB11

LS2_CC01 - LS2_CC12

LS2_CD01 - LS2_CD12

LS3_CD01 - LS3_CD06