Setting the attenuator threshold interlock

With the new OSE this shouldn't be needed anymore, but until then it is necessary to set an attenuator threshold interlock any time primary beam is being sent past the target dump.

Links

Threshold calculator form

Procedure to Set Interlock Threshold for RSS Attenuator

Attenuator Use Instructions