Opening EXP Area

Stop the beam.

Insert FC D1102 into beamline.

On the EXP Launch Page, go to Target-Hall/EXP Operator status page. Insert beam stop for required area.

On the MPS Operator page, turn E-Bends off.

On the PPS rack, turn the key for Linac AC to beam permit.

On the PPS rack, turn EXP vault ready for beam key to off.