Open/Close EXP area

Open

Stop Beam from running.

Insert FC D1102.

In the EXP Launch page, under status tab, open the T-Hall/EXP Operator page. Then insert beam stop for required area.

On the MPS Operator page, turn the E-Bends off.

On the PPS rack, turn the key for Linac ACS to power permit.

On the PPS rack, turn the EXP Vault Ready for Beam key to off.

Close

Turn EXP Vault Ready for Beam key to On.

Turn Linac ACS to beam permit.

On EXP page, remove beam stop that was inserted.

Remove FC D1102 from beam line.

Turn E-Bends On.

Start Chopper.