Sending beam to a new destination

Steps

Check the MPS Device Configuration Guideline for power limits and special notes

Calculate beam power

Configure chopper

Configure MPS

Coordinate with AP for whether cavities need monitoring

Calculate thresholds in Diag MPS pageUsing the new beamloss threshold configuration tool

Configure DCCTs if needed

Set beam inhibit mode

Send beam

Links

Limiting Primary Beam Power → This operator page has a lot of important information about the devices involved and how they work

FRIB MPS Device Configuration Guideline