When changing flux for FSEE, you'll want to first use the MHB and attenuators to make adjustments.

If you are going to change to a low flux around 1E3 pps/cm2, then you'll want to follow the steps below:

1. Switch FC_1102 cup to tetram reading on the FC Overview page. 2. Calculate the amount of flux needed on FC_2596 by using the calculator on the FSEE GUI. 3. Measure current on FC_2596 and record the current reading. Do the same on FC_1102. 4. Calculate the ratio between the FC_1102/FC_2596. Multiply this ratio and the desired up reading on FC_2596. This will be the reading you'll want to attain on FC_1102. 5. Put the beam back onto FC_1102 and adjust attenuators/the MHB to achieve the calculated value from the step before. 6. Insert the viewer to perform another uniformity measurement. 7. Send flux to the users /calibrate the jaws. 8. Beam is ready.