Recovering HPECR from Gate Valves Closing

If MPS tripped due to gate valves closing, please follow the HPECR recovery instructions:

On HPECR operator page, Open Gate Valve FE_ISRC2:BGV_D0675.

Go to Microwave Amp. in the 18GHz Microwave Transmitter section.

On the Microwave Amp page:

1. Reset all interlocks / safety interlocks

2. Turn on PLC commands
3. Reset all interlocks / safety interlocks again
4. Turn on BEAM power supply
5. Reset "RF OUTPUT Set point" to ZERO
6. Turn ON RF output
7. Recover the RF output power to where it was by 100V/step.
*Go back to the HPECR operator page, turn on both source high voltage and platform high voltage HVP D0652 and HVP D0677.
*Turn back on the acceleration column puller PSEL D0678.