Changing Between Beams Within A Cocktail

Beams changes within a cocktail may be completed quickly by changing the main field of the cyclotron and a limited number of changes to other beamline devices. The intention is to change the least number of devices while producing the same beam quality delivered to SEE.

Steps:

Run main probe in to 24“

This process could be done on FC2007, as long as the beam intensities for all beam species is within acceptable levels

Increase chopper duty cycle to 100%

Set the main field epsilon value to the new value

If the value is already logged/known, use that. Otherwise use the value from Analog Beams and add the offset for the pilot. e.g. Pilot is at -300 ppm, new beam expected at +5000 ppm, set field to +4700 ppm