Opening Area

Steps

Turn the Beam/Chopper off.

Go to Main Magnets page through FRIB Launch. Go go the BBS/FFS page. Turn Dipole D5578 off; this will take a moment to ramp down to 0 A.

On MPS Operator page, turn E-Bends off.

On the PPS machine, first turn the Linac ACS key to Beam Permit. Then, turn the key for Target RSS Ready For Beam to Off.

Operator goes to room and starts a survey for entire area, or specific spot if required.

After room is opened, on the PPS rack, flip the key for the opened room to Regulated Access.