Opening EXP Vault Area

Steps

Turn the Beam/Chopper off.

Inset FC D1102.

On the MPS Operator page, turn E-Bends off.

On the EXP Launcher, go to T-Hall/EXP Operator page. Insert Beam Stop for required area.

On the PPS rack, turn the key for Linac AC to Beam Permit. Then turn Experimental Vault ready for Beam key to off.