Opening EXP Vault Area

Steps

Turn the Beam/Chopper off

On the Main Magnets page, turn Dipole D5578 off on BBS/FFS tab; this will take a moment to ramp down to 0 A.

On the MPS Operator page, turn E-Bends off.

On the PPS rack, turn the Linac ACS key to Beam Permit.

On the PPS rack, turn the key for Target RSS Ready For Beam to Off.

Operator goes to room and starts a survey for entire area, or specific spot if required.

After room fully surveyed and opened, on the PPS rack, turn the key for the opened room to Regulated Access.