{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":2,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":174,"n_cols":13,"rows_kept":174,"cut":false,"hidden":false,"merged":[[10,0,10,9],[2,0,2,9],[55,0,55,9],[47,0,47,9],[42,0,42,9],[35,0,35,9],[26,0,26,9],[18,0,18,9],[84,0,84,9],[81,0,81,9],[77,0,77,9],[73,0,73,9],[68,0,68,9],[64,0,64,9],[126,0,126,9],[115,0,115,9],[110,0,110,9],[97,0,97,9],[92,0,92,9],[88,0,88,9]],"flags":["formulas_cached_only"]}
[]
["RUN","Date","Source","Gas",null,"HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["228Th source with a collimator"]
[18,"2009-06-12","228Th","Ar+Isobutane(10%) 1 atm",null,-260,-1,120,1000,160793,1.9999999999999998]
[19,"2009-06-12","228Th","Ar+Isobutane(10%) 1 atm",null,-260,-1,120,1000,160793,1.9999999999999998]
[{"$nulls":9},"total",3.9999999999999996]
[20,"2009-06-12","228Th","Ar+Isobutane(10%) 1 atm",null,-310,-1,600,1000,132574,1.6490021331774392,"Stopped at Nevent ~ 1.2 k"]
[21,"2009-06-12","228Th","Ar+Isobutane(10%) 1 atm",null,-310,-1,600,1000,160793,1.9999999999999998]
[{"$nulls":9},"total",3.649002133177439]
[]
["With a decoupling capacitor of 33.02 nF (c.f., 0.22 nF in RUN18-21)"]
[23,"2009-06-26","228Th","Ar+Isobutane(10%) 1 atm",null,-250,-0.9,120,1000,61745,0.7680060699159789]
[24,"2009-06-26","228Th","Ar+Isobutane(10%) 1 atm",null,-250,-0.9,120,1000,171465,2.1327420969818336]
[25,"2009-06-26","228Th","Ar+Isobutane(10%) 1 atm",null,-250,-0.9,120,1000,161999,2.0150006530135016]
[26,"2009-06-26","228Th","Ar+Isobutane(10%) 1 atm",null,-250,-0.9,120,1000,10693,0.13300330238256639]
[27,"2009-06-26","228Th","Ar+Isobutane(10%) 1 atm",null,-250,-0.9,120,1000,347072,4.317003849670073]
[{"$nulls":9},"total",9.365755971963953]
[]
["New gas cylinder, Over atomospheric pressure (1.1 atm) (c.f., RUN18-27 1atm), High Kathode voltage"]
[28,"2009-06-26","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,328316,4.083710111758596]
[29,"2009-06-26","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,45197,0.5621762141386751]
[30,"2009-06-26","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,535860,6.665215525551485]
[30.1,"2009-06-26","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,287400,3.5747824843121276]
[{"$nulls":9},"total",14.885884335760883]
[]
["RUN","Date","nEvents","Amplitude [0x]",null,"[0d]","TPC",null,null,"Data size [KB]","Event #","Memo"]
["On-board pulser calibration;  Mode = calibration"]
[32,"2009-07-01",2,"BF30",null,48944,"Connected",null,null,643,7.997860603384475]
[32.1,"2009-07-01",2,"BF00",null,48896,"Connected",null,null,643,7.997860603384475]
[32.2,"2009-07-01",2,"BE00",null,48640,"Connected",null,null,643,7.997860603384475]
[32.3,"2009-07-01",2,"BDC0",null,48576,"Connected",null,null,643,7.997860603384475]
[32.4,"2009-07-01",2,"BDD0",null,48592,"Connected",null,null,643,7.997860603384475]
[32.5,"2009-07-01",2,"BD00",null,48384,"Connected",null,null,643,7.997860603384475]
[]
["RUN","Date","Source","Gas",null,"HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["The pads were externally grounded with a load resistance of 11 MOhm, while the photoMOS of the FEC was switched off."]
[33,"2009-07-06","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,264264,3.287008762819277]
[34,"2009-07-06","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,241592,3.005006436847375]
[35,"2009-07-06","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,523301,6.509002257560963]
[35.1,"2009-07-06","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,240627,2.9930034267660903]
[{"$nulls":9},"total",15.794020883993706]
["RUN","Date","Source","Gas",null,"HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["The rate of the alpha source was increased by increasing the aperture of the collimator. The pads were externally grounded with a load resistance of 11 Mohm. The photoMOS of the FEC has been switched off."]
[36,"2009-07-07","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,523301,6.509002257560963]
[36.1,"2009-07-07","228Th","Ar+Isobutane(10%) 1.1 atm",null,-300,-2,360,1000,280665,3.491010180791452]
[{"$nulls":9},"total",10.000012438352416]
["RUN","Date","Source","Gas",null,"HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["Low pressure  run (P = ~0.7 atm)"]
[39,"2009-07-08","228Th","Ar+Isobutane(10%) 0.7 atm",null,-250,-2,360,1000,523301,6.509002257560963]
[39.1,"2009-07-08","228Th","Ar+Isobutane(10%) 0.7 atm",null,-250,-2,360,1000,280665,3.491010180791452]
[40,"2009-07-08","228Th","Ar+Isobutane(10%) 0.7 atm",null,-250,-2,360,1000,523301,6.509002257560963]
[40.1,"2009-07-08","228Th","Ar+Isobutane(10%) 0.7 atm",null,-250,-2,360,1000,227362,2.828008681969986]
[]
[]
["RUN","Date","Source","Gas",null,"HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["New Gas Ar+CO2(30%)"]
[41,"2009-07-09","228Th","Ar+CO2(30%) 1.1 atm",null,-400,-2,360,1000]
[42,"2009-07-09","228Th","Ar+CO2(30%) 1.1 atm",null,-500,-2,360,1000]
[43,"2009-07-09","228Th","Ar+CO2(30%) 1.1 atm",null,-525,-2,360,1000]
[44,"2009-07-09","228Th","Ar+CO2(30%) 1.1 atm",null,-550,-2,360,1000]
[45,"2009-07-09","228Th","Ar+CO2(30%) 1.1 atm",null,-500,-2,360,1000]
[{"$nulls":9},"total",19.337023377883366]
[]
["RUN","Date","Source","Gas",null,"HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["241Am  at P = ~1.0 atm"]
[46,"2009-07-10","241Am","Ar+Isobutane(10%) 1.0 atm",null,-260,-2,120,1000,523301,6.509002257560963]
[46.1,"2009-07-10","241Am","Ar+Isobutane(10%) 1.0 atm",null,-260,-2,120,1000,280665,3.491010180791452]
[{"$nulls":9},"total",10.000012438352416]
["241Am  at P =  ~0.65 atm"]
[47,"2009-07-10","241Am","Ar+Isobutane(10%) 0.65 atm",null,-210,-2,120,1000,523301,6.509002257560963]
[47.1,"2009-07-10","241Am","Ar+Isobutane(10%) 0.65 atm",null,-210,-2,120,1000,280665,3.491010180791452]
[{"$nulls":9},"total",10.000012438352416]
["RUN","Date","Source","Gas",null,"HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["241Am  in He+CO2(10%) at P = ~1.0 atm"]
[48,"2009-07-20","241Am","He+CO2 (10%) 1.0 atm",null,-350,-2,120,1000,80396,0.999993780823792]
[]
["RUN","Date","Source","Gas","uMega ID","HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["241Am  in Ar+Isobutane(10%), P = ~0.5 atm"]
[50,"2009-07-28","241Am","Ar+Isobutane(10%) 0.5 atm","1b",-210,-1,120,1000,523301,6.509002257560963]
[50.1,"2009-07-28","241Am","Ar+Isobutane(10%) 0.5 atm","1b",-210,-1,120,1000,280665,3.491010180791452]
[{"$nulls":9},"total",10.000012438352416]
["241Am  in He+CO2(10%), P = ~1.0 atm"]
[51,"2009-07-28","241Am","He+CO2(10%) 1.0 atm","1b",-250,-2,120,1000,401983,5.000006219176208]
[]
["241Am  in He+CO2(15%), P = ~1.0 atm"]
[52,"2009-07-28","241Am","He+CO2(15%) 1.0 atm","1b",-270,-2,120,1000,523301,6.509002257560963]
[52.1,"2009-07-28","241Am","He+CO2(15%) 1.0 atm","1b",-270,-2,120,1000,120354,1.4970054666558867]
[{"$nulls":9},"total",8.00600772421685]
["241Am  in He+CO2(20%), P = ~1.0 atm"]
[53,"2009-07-29","241Am","He+CO2(20%) 1.0 atm","1b",-320,-2,120,1000,523301,6.509002257560963]
[53.1,"2009-07-29","241Am","He+CO2(20%) 1.0 atm","1b",-320,-2,120,1000,280665,3.491010180791452]
[{"$nulls":9},"total",10.000012438352416]
["241Am  in He+CO2(30%), P = ~1.0 atm"]
[54,"2009-07-29","241Am","He+CO2(30%) 1.0 atm","1b",-350,-2,120,1000,523301,6.509002257560963]
[54.1,"2009-07-29","241Am","He+CO2(30%) 1.0 atm","1b",-350,-2,120,1000,280665,3.491010180791452]
[{"$nulls":9},"total",10.000012438352416]
["RUN","Date","Source","Gas","uMega ID","HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["electronics calibration"]
[70,"2009-08-31","pulser","NA",null,0,0,120120120120,null,null,0.924,"3FFF, 3C00, 3A00, 3800, 3400, 3000"]
[71,"2009-08-31","pulser","NA",null,0,0,120120120120,null,null,0.924,"BFFF, BF00, BE00, BC00, B800, B000","electronics disconnected from chamber"]
[72,"2009-08-31","pulser","NA",null,0,0,120120120120,1000,null,0.924,"BF80, BF00, BE80, BE00, BD7F, BD00"]
[73,"2009-08-31","pulser","NA",null,0,0,120120120120,1000,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00"]
[74,"2009-08-31","pulser","NA",null,0,0,600120120120,null,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00"]
[75,"2009-08-31","pulser","NA",null,0,0,600120120120,null,null,0.924,"BF80, BF00, BE80, BE00, BD7F, BD00"]
[76,"2009-09-02","pulser","NA",null,0,0,600600600600,null,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00"]
[77,"2009-09-02","pulser","NA",null,0,0,600600600600,null,null,0.924,"aborted"]
[78,"2009-09-02","pulser","NA",null,0,0,600600600600,null,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00"]
[]
[]
["RUN","Date","Source","Gas","uMega ID","HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["gain test with 55Fe source"]
[84,"2009-09-08","55Fe","He+CO2(10%) 1.0 atm","1b",-400,-2,120,1000,null,0.05]
[85,"2009-09-08","55Fe","He+CO2(10%) 1.0 atm","1b",-450,-2,120,1000,null,0.05]
[]
["RUN","Date","Source","Gas","uMega ID","HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["gain test with 241Am source"]
[88,"2009-09-09","241Am","He+CO2(10%) 1.0 atm","1b",-200,-1,120,1000,null,1,"nice tracks"]
[89,"2009-09-09","241Am","He+CO2(10%) 1.0 atm","1b",-200,-2,120,1000,null,0.05,"crap"]
[90,"2009-09-09","241Am","He+CO2(10%) 1.0 atm","1b",-330,-2,120,1000,null,0.05,"crap"]
[91,"2009-09-09","241Am","He+CO2(10%) 1.0 atm","1b",-300,-1.5,120,1000,null,0.05]
[92,"2009-09-09","241Am","He+CO2(10%) 1.0 atm","1b",-200,-1,120,1000,null,0.05,"nice tracks"]
[93,"2009-09-09","241Am","He+CO2(10%) 1.0 atm","1b",-220,-1,120,1000,null,0.05,"nice tracks"]
[94,"2009-09-09","241Am","He+CO2(10%) 1.0 atm","1b",-240,-1,120,1000,null,0.05,"nice tracks"]
[95,"2009-09-09","241Am","He+CO2(10%) 1.0 atm","1b",-260,-1,120,1000,null,0.05,"nice tracks - check if saturated"]
[96,"2009-09-09","241Am","He+CO2(10%) 1.0 atm","1b",-280,-1,120,1000,null,0.05,"umega tripped - strip 4 hot"]
["RUN","Date","Source","Gas",null,"HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
[]
[97,"2009-09-11","pulser","NA","2b",0,0,120120120120,1000,null,0.924,"BF80, BF00, BE80, BE00, BD7F, BD00","disconnected adapter board"]
[98,"2009-09-11","pulser","NA","2b",0,0,120120120120,1000,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","connected adapter board"]
[99,"2009-09-11","pulser","NA","2b",0,0,120120120120,1000,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","disconnected adapter board"]
[100,"2009-09-11","pulser","NA","2b",0,0,120120120120,1000,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","connected adapter board"]
[]
[101,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-200,-1,120,1000,null,0.05,"double tracks"]
[102,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-300,-1,120,1000,null,0.05,"adc range saturated"]
[103,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-350,-1,120,1000,null,0.05,"adc range saturated"]
[104,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1.5,120,1000,null,0.05,"broad track"]
[105,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,120,1000,null,0.05,"good tracks"]
[106,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-2,120,1000,null,0.05,"good tracks"]
[{"$nulls":11},"sparking began at a cathode voltage of -2.2kV"]
[107,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,240,1000,null,0.05]
[108,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,360,1000,null,0.05]
[109,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,600,1000,null,0.05,"maximum adc range"]
[]
[110,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-200,-1,600,1000,null,0.05]
[111,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,600,1000,null,0.05]
[112,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-300,-1,600,1000,null,0.05]
[113,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-350,-1,600,1000,null,0.05]
[114,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-400,-1,600,1000,null,0.05,"BAD!!!! sparking??"]
[]
[115,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,600,100,null,0.05]
[116,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,600,500,null,0.05]
[117,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,600,1000,null,0.05]
[118,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,600,1500,null,0.05]
[119,"2009-09-11","241Am","He+CO2(10%) 1.0 atm","2b",-250,-1,600,2000,null,0.05]
[]
[120,"2009-09-11","pulser","NA","2b",0,0,600,100,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","connected adapter board"]
[121,"2009-09-11","pulser","NA","2b",0,0,600,500,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","connected adapter board"]
[122,"2009-09-11","pulser","NA","2b",0,0,600,1000,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","connected adapter board"]
[123,"2009-09-11","pulser","NA","2b",0,0,600,1500,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","connected adapter board"]
[124,"2009-09-11","pulser","NA","2b",0,0,600,2000,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","connected adapter board"]
[125,"2009-09-11","pulser","NA","2b",0,0,240,1000,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","connected adapter board"]
[126,"2009-09-11","pulser","NA","2b",0,0,360,1000,null,0.924,"3F80, 3F00, 3E80, 3E00, 3D7F, 3D00","connected adapter board"]
[]
[]
[127,"2009-09-18","241Am","P10 1.0atm","2b",-300,-2,600,1000,null,0.05]
[128,"2009-09-18","241Am","P10 1.0atm","2b",-300,-2,600,1000,null,0.05]
[129,"2009-09-18","241Am","P10 1.0atm","2b",-275,-1,600,1000,null,0.05]
[]
[]
[130,"2009-09-28","241Am","He+CO2(5%) 1.0 atm","2b",-200,-1,600,1000,null,0.05,"BAD!!!!"]
[131,"2009-09-28","241Am","He+CO2(5%) 1.0 atm","2b",-175,-1,600,1000,null,0.05,"good tracks"]
[]
[132,"2009-09-29","241Am","He+CO2(7%) 1.0 atm","2b",-175,-1,600,1000,null,0.05]
[133,"2009-09-29","241Am","He+CO2(7%) 1.0 atm","2b",-200,-1,600,1000,null,0.05]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}