{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":12,"rows_kept":10,"cut":false,"hidden":false,"merged":[[2,0,2,9],[5,0,5,9]],"flags":["formulas_cached_only"]}
[]
["RUN","Date","Source","Gas","Umegas ID","HV umegas [V]","Kathode [kV]","ADC full scale range [fC]","Peaking time [ns]","Data size [KB]","Event # [k]","Memo"]
["241Am  in He+CO2(30%), P = ~1.0 atm"]
[201,"2009-11-16","241Am","He+CO2(30%) 1.0 atm","2b",-480,-2,600,1000,411630,5.119999004931806]
[{"$nulls":9},"total",5.119999004931806]
["241Am  in He+CO2(30%), P = ~1.0 atm"]
[202,"2009-11-16","241Am","He+CO2(30%) 1.0 atm","2b",-480,-4,600,200,411630,5.119999004931806]
[{"$nulls":9},"total",5.119999004931806]
[203,"2009-11-16","241Am","He+CO2(30%) 1.0 atm","2b",-580,-4,120,200,411630,5.119999004931806]
[{"$nulls":9},"total",5.119999004931806]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}