{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
["Name","Material","dimension","Qty","For"]
["Plate","Al","8.00\" x 16.5\"",1,"Front panel"]
["Plate","Al","16.88\" x 16.5\"",2,"Top/bottom"]
["Plate","Al","16.88\" x 7.764\"",2,"Side"]
["Stick","Al","(1\" x 1/2\")fix x 16\"",1,"Pipe fixer"]
["Stick","Al","(1\" x 1/2\")fix x 12\"",1,"Pipe fixer"]
["Stick","Al","(1\" x 1/2\")fix x 7.764\"",3,"Support#1"]
["Stick","Al","(1/2\" x 1/2\")fix x 7.764\"",4,"Support#2"]
["NPS Nipple","SUS","1/4\", NPT fitting, 2\" length",1,"Section A"]
["NPS Nipple","SUS","1/4\", NPT fitting, 3\" length",1,"Section A"]
[" NPS Coupling","SUS","1/4\", NPT fitting",1,"Section A"]
["NPS Nipple","SUS","1/4\", NPT fitting, 4~5\" length",3,"Section B"]
["NPS Pipe","SUS","1/4\", 4\" length",1,"Section B"]
["NPS Tee","SUS","1/4\", weld fitting",1,"Section B"]
["NPS 90 deg elbow","SUS","1/4\", weld fitting",1,"Section B"]
["NPS Nipple","SUS","1/4\", NPT fitting, 2\" length",3,"Section C1/C2"]
["NPS 90 deg elbow","SUS","1/4\", weld fitting",5,"Section C1/C2"]
["NPS Pipe","SUS","1/4\", 3\" length",5,"Section C1/C2"]
["NPS cross","SUS","1/4\", weld fitting",1,"Section C1/C2"]
["NPS Nipple","SUS","1/4\", NPT fitting, 3~4\" length",1,"Section C1/C2"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}