{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":59,"n_cols":16,"rows_kept":59,"cut":false,"hidden":false,"merged":[[2,9,2,13]],"flags":["formulas_cached_only"]}
["Purchase List "]
[]
[{"$nulls":9},"Quote"]
["Item","Qty","Stock in NSCL","Qty buy",null,"Company","Product name","Specification","Link","Request ","Date ","Lead time","Price ($/EA)","Price ($)","Purchase order (Req. ID, Req Date, Requestor)","Received date"]
["N2 bottle (bottle rent = 0.5 year)",1,0,1,null,"PURITY CYLINDER GASES INC",null,"Gas = $38.55/bottle; Cylinder rent =  $0.36/day",null,"DS","2009-06-26","1-2 d",104.25,104.25,"43484, 7/13/2009, DS"]
["Excess flow valve",1,0,1,"section C(1)",null,"MLV-6015-SA +6295-A","VLVNPTF 4 SLPM",null,"KC","2009-05-29","2 wk",902.81,902.81]
[null,1,0,1,null,null,"MLV-6016-SA +6295-C","VLVNPTF 100SLPM",null,"KC","2009-05-29","2 wk",721,721]
[null,1,0,1,null,null,"MLV-6017-SA +6295-F ","VLVNPTF 100SLPM",null,"KC","2009-05-29","2 wk",576.56,576.56]
[null,1,0,1,null,"Matheson","6295-C","EXCESS FLOW VLV, 20LPM @ 1000PSIG, 4LPM @ 30PSIG","here","DS","2009-05-29","3 d",670,670,"43454, 7/7/2009, DS","2009-07-15"]
["Flash arrestor",1,0,1,"section C(1)","Matheson","6103A-F","FLASH ARRESTOR BRASS FLAMMABLES 1/4 FNPT","here","DS","2009-05-29","3 d",117,117,"43454, 7/7/2009, DS","2009-07-15"]
["Adapter KF16->1/4\" NPT(F)",3,0,3,"section C(3)","Lesker","QF16XFNPT4","SS304",null,"DS",null,null,24,72,"43477, 7/8/2009, DS","2009-07-10"]
["Adapter KF16->1/4\" NPT(M)",6,0,6,"section B(2)/ section C(4)","Lesker","QF16XMNPT4","SS304",null,"DS",null,null,45,270,"43477, 7/8/2009, DS","2009-07-10"]
["Adapter KF25->1/4\" NPT(F)",0,0,0,null,"Lesker","QF25XFNPT4","SS304",null,"DS",null,null,27,0]
["Adapter KF25->1/4\" NPT(M)",1,0,1,"section A(1)","Lesker","QF25XMNPT4","SS304",null,"DS",null,null,47,47,"43477, 7/8/2009, DS","2009-07-10"]
["Adapter KF25->3/4\" NPT(M)",2,0,2,"vent at the wall (1)/ Pressure relief vent (1)","Lesker","QF25XMNPT12","SS304",null,"DS",null,null,55,110,"43477, 7/8/2009, DS","2009-07-10"]
["Centering KF16",12,12,0,null,"Lesker","QF16-075-SRV",null,null,"DS",null,null,6,0]
["Centering KF25",5,5,0,null,"Lesker","QF25-075-SRV",null,null,"DS",null,null,7,0]
["Cast clamp KF16",12,12,0,null,"Lesker","QF16-075-C","Al",null,"DS",null,null,6,0]
["Cast Clamp KF25",5,5,0,null,"Lesker","QF25-100-C","Al",null,"DS",null,null,8,0]
["1/4\" NPT(M)-1/4\" VCO(Body)",1,0,1,"section A","Swagelok","SS-4-VCO-1-4 ","316 SS VCO O-Ring Face Seal Fitting, Male NPT Connector, 1/4 in. VCO Fitting x 1/4 in. MNPT",null,"DS",null,"3 d",10.4,10.4,"43467, 7/8/2009, DS","2009-07-22"]
["1/4\" NPT(F)-1/4\" VCO(Body)",1,0,1,"section A","Swagelok","SS-4-VCO-7-4 ","316 SS VCO O-Ring Face Seal Fitting, Female NPT Connector, 1/4 in. VCO Fitting x 1/4 in. FNPT",null,"DS",null,"3 d",13.1,13.1,"43467, 7/8/2009, DS","2009-07-22"]
["VCO(F)-VCO(F) 1/4\" cable 30 cm (from the metering valve to the flowmeter)",1,0,1,"section A","Swagelok","SS-VJ4VF4VF4-30CM",null,null,"DS",null,"1 wk",113.85,113.85,"43467, 7/8/2009, DS","2009-07-22"]
["Coupling NPT 1/4\"",1,0,1,"section A","Swagelok","SS-4-HCG","SUS",null,"DS",null,"1 wk",9.7,9.7,"43467, 7/8/2009, DS","2009-07-22"]
["Tube socket  weld fitting OD1/2\"-NPT1/4\"(M)",2,0,2,"section A(1)/ section C(1)","Swagelok","SS-8-TSW-1-4","SUS",null,"DS",null,"1 wk",11,22,"43467, 7/8/2009, DS","2009-07-22"]
["Weld KF16 flange",7,0,7,"section A(1)/ section B(3)/ section C(3)","Lesker","QF16-050-SS","SUS",null,"DS",null,null,10,70,"43477, 7/8/2009, DS","2009-07-10"]
["Weld fitting 90 deg radius ELBOW OD1/2\"",6,0,6,"section B(1)/ section C(5)","Lesker","G-2WC-050","SUS",null,"DS",null,null,12,72,"43477, 7/8/2009, DS","2009-07-10"]
["Weld fitting TEE OD1/2\"",2,0,2,"section B(1)/ section C(1)","Lesker","G-7W-050","SUS",null,"DS",null,null,30,60,"43477, 7/8/2009, DS","2009-07-10"]
["Weld fitting Cross OD1/2\"",1,0,1,"section C(1)","Lesker","G-9W-050","SUS",null,"DS",null,null,58,58,"44016, 8/6/2009, DS"]
["KF16 overpressure ring",10,5,5,"section A(3)/ section B(3)/ section C(4)","Swagelok"," JNWPR16","SUS",null,"DS",null,"1 wk",5.78,28.900000000000002,"43467, 7/8/2009, DS","2009-08-04"]
["Weld KF25 flange",2,0,2,"SS tube to the vent (2)","The pump works Inc."," NW25-100-LF","SUS",null,"DS",null,null,15.5,31,"43465, 7/8/2009, DS","2009-07-28"]
["SS flexible tube",1,0,1,"Pressure relief vent -> Pump exhaust","Swagelok","JNW2FH25-36.00","304 SS KF Flexible Hose, KF 25 Flange Size x 36 in. (914 mm) Length",null,"DS",null,"1 d",120,120,"43467, 7/8/2009, DS","2009-07-24"]
["NW25 tee",1,1,0,"Pressure relief vent -> Pump exhaust (1) ","Lesker","QF25-100-T","SS",null,"DS",null,null,72,0]
["NW16 tee",1,1,0,"section A","Lesker","QF16-075-T","SS",null,"DS",null,null,66,0]
["SS tube",1,1,0,"Piping","Swagelok","304L-T8-W-049-20","Outer diameter 1/2\", length 6m",null,"DS",null,null,207.8,0]
["H2 sensor",1,0,1,null,"ENMET","EX-5100",null,null,"KC","2009-05-29",null,2040,2040]
["H2 bottle",1,0,1,null,"PURITY CYLINDER GASES INC","Size 1A (213 CF) ","Research Grade Hydrogen 99.9999          ",null,"KC","2009-05-29",null,262,262]
[null,1,0,1,null,"PURITY CYLINDER GASES INC","Size 2 (76 CF) ","Research Grade Hydrogen 99.9999            ",null,"KC","2009-05-29",null,167,167,"43484, 7/13/2009, DS","2009-07-27"]
[null,1,0,1,null,"PURITY CYLINDER GASES INC","Size 3 (30 CF) ","Research Grade Hydrogen 99.9999 ",null,"KC","2009-05-29",null,148,148]
["H2 regulator",1,0,1,null,"PURITY CYLINDER GASES INC","MREG-1233-XX +3180-350",null,null,"KC","2009-05-29","2 wk",719.25,719.25,"43484, 7/13/2009, DS"]
["N2 flowmeter",1,0,1,null,"Matheson","E 1-4G201-E800 ","SLPM(N2) = 2.47-46 (Expected 48 SLPM)",null,"DS",null,"2 wk",302,302]
[null,1,0,1,null,"Swagelok","VAF-G2-15M-1-0","SLPM(N2) = 8.3 - 83 (Expected 48 SLPM)",null,"DS",null,"3 wk",303.71,303.71,"43467, 7/8/2009, DS","2009-08-04"]
["Pump flowmeter",1,0,1,null,"Matheson","E 1-4G201-E300 ","SLPM(H2) = 0.099 - 2.5 (Expected < ~1.8 SLPM)",null,"DS",null,"2 wk",302,302]
[null,1,0,1,null,"Swagelok","VAF-G2-06M-1-0","SLPM(H2) = 0.4 - 4.2 (Expected < ~1.8 SLPM)",null,"DS",null,"3 wk",303.71,303.71,"43467, 7/8/2009, DS","2009-07-22"]
[null,1,0,1,null,"Swagelock","VAF-G2-07M-1-0","SLPM(H2) = 1.1 - 11 (Expected < ~1.8 SLPM)",null,"DS",null,"3 wk",303.71,303.71]
["Meetering valve",1,0,1,null,"Swagelock","SS-4MG2-MH ","SS Medium-Flow Metering Valve, 1/4 in. MNPT, Vernier Handle",null,"DS",null,"5 days",138.7,138.7]
[null,1,0,1,null,"Swagelok","SS-4MA2-MH","SS Medium-Flow Metering Valve, 1/4 in. MNPT, Vernier Handle, Angle type",null,"DS",null,"1 wk",126.06,126.06,"43467, 7/8/2009, DS","2009-07-22"]
["Gate valves",3,0,3,null,"Matheson","FM4374A","VALVE DIAPHRAGM MULTITURN SSTEEL, 1/4NPTF X 1/4NPTM",null,"DS",null,"3 days",183,549]
[null,3,0,3,null,"Swagelok","SS-DSM4F4A","SS High-Purity High-Pressure Angle-Pattern Diaphragm-Sealed Valve, 1/4 in. MNPT x 1/4 in. FNPT, Round Handle",null,"DS",null,"3 days",191.2,573.5999999999999,"43467, 7/8/2009, DS","2009-07-22"]
["Gas handler lines",2,0,2,null,"Swagelok","JNW2FH16-36.00","Vacuum flexible hose, SS, KF16, 36\"",null,"DS",null,"3 wk",123,246,"43467, 7/8/2009, DS","2009-08-04"]
["Chamber lines",2,0,2,null,"Swagelok","SS-FJ4VF4PM4-120 HOSE","stainless steel interior, 120 in, 1/4\" VCO to 1/4\" NPT",null,"KC",null,"2 wk",179.85,359.7,"43467, 7/8/2009, DS","2009-07-22"]
["Foreline trap for the rotary pump",1,0,1,"Vuccum pump","Edwards","A13305000","FL20K foreline trap",null,"DS",null,"a few days",393,393,"R43478, 7/8/2009, DS","2009-07-10"]
["Gas filter",1,0,1,"Gas filter","Swagelock","SS-4F2-05","NPT 1/4\", 0.5 um ",null,"DS",null,"1 wk",75.24,75.24]
[null,null,0,0,null,"Swagelok","SS-4F2-2","NPT 1/4\", 2 um ",null,"DS",null,"1 wk",68.97,68.97,"43467, 7/8/2009, DS","2009-07-22"]
["NW16 Elbow",1,1,0,"Gas filter","Lesker","QF16-075-E90","SS",null,"DS",null,null,42,0]
[]
["total",{"$nulls":12},7395.200000000001]
[]
["swagelok",{"$nulls":12},2299.6999999999994]
["lesker",{"$nulls":12},759]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}