{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["CENBG","MAYA","MSU"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":3,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"CENBG","index":0,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Category","parameters","Value","Unit","Remark"]
[]
["Detector Information:"]
["chamber type :",null,null,null,"cylindric, rectangle, quarre"]
[]
["size:","diameter",null,"cm"]
[]
[null,"width",20,"cm"]
[null,"length",20,"cm"]
[null,"heigth",null,"cm"]
["Readout plane",null,"MicroMegas / Gem",null,"Gem, Micromegas, Wire chamber"]
["Dead Zone",null,null,"%"]
["Pad size","length",2,"mm"]
[null,"width",2,"mm"]
["number of Pad",null,10000]
["gaz",null,"P10"]
["drift speed"]
["drift Time",null,10,"µs"]
["environment","Electric Field",null,"V/cm"]
[null,"Magnetic Field",null,"Tesla"]
[null,"Vacuum",null,"TOR"]
[null,"Pressure",null,"mBar"]
[null,"temperature",25,"°C"]
[null,"Temp. Variation",null,"°K"]
["mean event rate",null,1,"Bq ","Bequerel"]
["number of touched pads/event",null,10,"%"]
[]
["Physics"]
["Type of reaction"]
["detector Gain"]
["Minimum ionization particles Energy"]
["Signal Polarity",null,"Negative"]
["minimum threshold",null,1,"fC"]
[]
["System"]
["Experiment Place",null,"GANIL / MSU"]
["Foreseen Acquisition",null,"GANIL / MSU"]
["Existing system",null,"No"]
["Multiplicity",null,"No Need"]
["Trigger level"]
["Information type",null,"Energy, Time",null,"Waveform, Energy, Time"]
["TimeStamp resolution",null,"10 ns"]
["Jitter",null,"1 ns"]
["electronic environment",null,"extern",null,"Magnetic, Vacuum"]
["dead Time",null,"< 1","ms"]

{"sheet":"MAYA","index":1,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Category","parameters","Value","Unit","Remark"]
[]
["Detector Information:"]
["chamber type :",null,"rectangle",null,"cylindric, rectangle, quarre"]
[]
["size:","diameter",null,"cm"]
[]
[null,"width",20,"cm"]
[null,"length",20,"cm"]
[null,"heigth",30,"cm"]
["Readout plane",null,"Micromegas, Wire",null,"Gem, Micromegas, Wire chamber"]
["Dead Zone",null,0,"%"]
["Pad size","length",2,"mm"]
[null,"width",2,"mm"]
["number of Pad",null,10000]
["gaz",null,"ALL available"]
["drift speed",null,"200ns/cm to 2µs/cm"]
["drift Time",null,"4µs to 50µs","µs"]
["environment","Electric Field",null,"V/cm"]
[null,"Magnetic Field","No","Tesla"]
[null,"Vacuum","2008-06-10","TOR"]
[null,"Pressure","20mb tp 2 atm","mBar"]
[null,"temperature","ambiant","°C"]
[null,"Temp. Variation",5,"°K"]
["mean event rate",null,"100 to 1000","Bq ","Bequerel"]
["number of touched pads/event",null,"1 to 10","%"]
[]
["Physics"]
["Type of reaction"]
["detector Gain"]
["Minimum ionization particles Energy"]
["Signal Polarity",null,"Pos; Neg"]
["minimum threshold",null,"noise level","fC"]
[]
["System"]
["Experiment Place",null,"GANIL / JAPON / TRIUMF "]
["Foreseen Acquisition",null,"GANIL"]
["Existing system",null,"No"]
["Multiplicity",null,"YES"]
["Trigger level",null,2]
["Information type",null,"Waveform, Energy, Temps",null,"Waveform, Energy, Time"]
["TimeStamp resolution",null,10,"ns","48 bits"]
["Jitter",null,2,"ns"]
["electronic environment",null,null,null,"Magnetic, Vacuum"]
["dead Time",null,"< 1","ms"]

{"sheet":"MSU","index":2,"n_rows":45,"n_cols":5,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Category","parameters","Value","Unit","Remark"]
["updated: A. Bickley, June 3, 2008"]
["Detector Information:"]
["chamber type :",null,"Cylindric",null,"cylindric, rectangle, quarre"]
[]
["size:","diameter",70,"cm"]
[]
[null,"width",null,"cm"]
[null,"length",120,"cm"]
[null,"heigth",null,"cm"]
["Readout plane",null,"Gem, Wire",null,"Gem, Micromegas, Wire chamber"]
["Dead Zone",null,4,"cm diameter"]
["Pad size","length",5,"mm"]
[null,"width",5,"mm"]
["number of Pad",null,10000]
["gaz",null,"ALL available"]
["drift speed",null,"200ns/cm to 2µs/cm"]
["drift Time",null,"4µs to 50µs","µs"]
["environment","Electric Field",null,"V/cm"]
[null,"Magnetic Field","0-2","Tesla"]
[null,"Vacuum","air","TOR"]
[null,"Pressure","0.2-1atm","mBar"]
[null,"temperature","ambiant","°C"]
[null,"Temp. Variation",5,"°K"]
["mean event rate",null,"100 to 1000","Bq ","Bequerel"]
["number of touched pads/event",null,"1 to 25","%"]
[]
["Physics"]
["Type of reaction",null,"transfer, resonance, fission and heavy ion reactions"]
["detector Gain"]
["Minimum ionization particles Energy"]
["Signal Polarity",null,"Pos; Neg"]
["minimum threshold",null,"noise level","fC"]
[]
["System"]
["Experiment Place",null,"MSU "]
["Foreseen Acquisition",null,"MSU "]
["Existing system",null,"No"]
["Multiplicity",null,"YES"]
["Trigger level",null,2]
["Information type",null,"Waveform, Energy, Temps",null,"Waveform, Energy, Time"]
["TimeStamp resolution",null,10]
["Jitter",null,2]
["electronic environment",null,"magnetic field, air",null,"Magnetic, Vacuum"]
["dead Time",null,"< 1","ms"]