Networks(WIP)

You can tell which network something is on based on a sticker at the bottom left of the screen. OFC machines run Windows 11 and the others run the Debian 12 distro of Linux.

FTC (FRIB Totally Cool)

This network controls/monitors the FRIB beamline from the sources up to the Transfer Hall.

EXP (Experimental)

This network controls/monitors the FRIB beamline from the Transfer Hall to the S1, S2, S3, and N4 experimental vaults.

CTL (Controls)

This netowkr monitors the ReA beamline.

OFC (Office)

This is an office machine that is normally used for more bureaucratic tasks.