Pumps

Info

Vacuums are essential to the beamline, as they are what keeps each section clear of any gas or residual particles out. Without them, beam would not be able to be delivered safely. In order the create a nearly complete vacuum within the beamline, there are multiple different types that are required. Each of the main ones that you may here often are listed below with their own pages.

Turbo Pumps

Ion Pumps

Scroll

Roughing Pumps

Tips/Notes

Location

Devices/PV's

Personnel

Brandon Ewert

Joshua Willard

Tim Embury

Mike Welton

Shane: I think enough can be said about pumps as a larger entity to fill this out more

Shane: Don't like the page names, something like “ion” is too general

Shane: We can quantify “nearly complete vacuum” to like e-9 Torr

Personnel page i still don't like but it should differentiate different beam lines for Kyle and Blake