Super Conducting Magnets(SCM)

Info

Similar to the dipoles in FS1, the super conducting magnets are also used to alter the beams path, however these magnets are stronger than the dipoles. With the increased strength, they are used to bend the beam after it leaves LS2 and moves through FS2 since the by the time beam leaves LS2 it has done most of its acceleration.

Tips/Notes

Location

Devices/PV's

Personnel