Performing a CSD

Open the Physapps launcher

Switch to the Apps tab, “All”

Open Charge State Distribution Scan

Select source (selection popup may default to the upper left screen)

Adjust range and gap if desired

Click Scan start

Do not close the application until the scan is complete

When done, click Save the scan and save in the default folder

Showing reference lines

Comparing to previous scans