Search and Evict

Before beam can be sent into an area that has been previously open to workers, operators must secure this area and evict any personnel found in the area. This is to prevent unnecessary exposure from beam induced radiation or, in certain areas like the FRIB linac tunnel, from x-ray radiation.

Throughout each area, there are a series of arm buttons placed in strategic locations along with gates/doors with associated switches. When securing an area, operators must go through and correctly push the arm buttons and close the doors and/or gates in the correct sequence as they search for any occupants. When this is done correctly, this will signal to the PPS that the area has been secured and is ready for beam operation.

An operator must have either attained the relevant competencies on Enterprise or be escorted by a fully trained operator to perform a search and evict procedure.

FRIB

Linac Tunnel

Enterprise Competency: Perform an FRIB Tunnel Search and Evict

Staffing: Minimum of two (2) fully trained and authorized personnel

Equipment: Validated Linac Tunnel ACS, hardhat, inspection mirror (optional), padlock/key #48, radio

Documentation: Search and Evict Procedure for FRIB Linac Tunnel - Credited Administrative Control with ESH Impact

Target Hall (B605A & B605)

Enterprise Competency: Perform an FRIB Target Hall Search and Evict

Staffing: Minimum of two (2), at least one of whom is fully trained and authorized

Equipment: Validated Target Facility ACS, hardhat, safety glasses, radio

Documentation: Search-and-Evict Procedure for the FRIB Target Hall (B605A and B605) – Credited Administrative Control with ESH Impact

VPS & ARIS

Enterprise Competency: Perform an FRIB VPS Search and Evict

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated Target Facility ACS, radio, padlocks/keys #26, #27, #28, and #57

Documentation: Search-and-Evict Procedure for Vertical Pre-Separator and ARIS Areas – Credited Administrative Control with ESH Impact

Transfer Hall (1500TH)

Enterprise Competency: Perform an FRIB Transfer Hall Search and Evict

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated Transfer Hall ACS, radio

Documentation: Search-and-Evict Procedure for the FRIB Transfer Hall (1500TH) – Credited Administrative Control with ESH Impact

Mechanical Areas

Room 1603

Enterprise Competency: FRIB Mechanical Room 1603 Search-and-Evict

Staffing: Minimum of two (2) personnel, one of whom is fully trained and authorized

Equipment: Padlocks/Keys #3 and #57, radio

Documentation: Search-and-Evict Procedure for Mechanical Room 1603 – Credited Administrative Control with ESH Impact

NCU Rooms (B601, SB601, & SB602/SSB603)

Enterprise Competency: FRIB NCU Rooms (B601, SB601, and SB602/SSB603) Search-and-Evict

Staffing: Minimum of two (2) personnel, one of whom is fully trained and authorized

Equipment: Padlocks/Keys #3 and #57, radio

Documentation: Search-and-Evict Procedure for Non-Conventional Utility Areas – Credited Administrative Control with ESH impact

Experimental Vaults

N4

Enterprise Competencies:

Unsecure/Re-secure the N4 Vault During User Operations

Act as Qualified For Task (QFT) worker, DC systems

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated N4 ACS, Personal HV LOTO Padlock, radio

Documentation:

N4/LEBIT Platform High Voltage Lock Out Tag Out Procedure

Search-and-Evict Procedure for N4 – Credited Administrative Control with ESH Impact

S1

Enterprise Competency: Perform and S1 Experimental Vault Search-and-Evict

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated S1 ACS, radio

Documentation: Search-and-Evict Procedure for S1 Experimental Vault – Credited Administrative Control with ESH Impact

S2/S3

Enterprise Competency: Perform an S2/S3 Experimental Vaults Search-and-Evict

Staffing: Minimum of two (2) personnel for the S3 basement and sub-basement levels, one of whom is fully trained; minimum of one (1) fully trained and authorized person for all other areas in the vaults

Equipment: Validated S2/S3 ACS, radio

Documentation: Search-and-Evict Procedure for S2 and S3 – Credited Administrative Control with ESH Impact

ReA

ReA3 RFQ Area

Enterprise Competency: Perform RFQ Area on ReA3 Platform Search and Evict

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated ReA ACS, radio

Documentation: Search-and-Evict Procedures for RFQ Area on ReA3 Platform – Credited Administrative Control with ESH Impact

ReA3 SRF Area

Enterprise Competency: Perform SRF Area on ReA3 Platform Search and Evict

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated ReA ACS, radio

Documentation: Search-and-Evict Procedures for Superconducting Radio Frequency (SRF) Area on ReA3 Platform – Credited Administrative Control with ESH Impact

ReA6 Accelerator Vault

Enterprise Competency: Perform ReA6 Accelerator Vault Search and Evict

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated ReA ACS, radio

Documentation: Search-and-Evict Procedure for ReA6 Accelerator Vault – Credited Administrative Control with ESH Impact

ReA6 Experimental Vault

Enterprise Competency: Perform ReA6 Experimental Vault Search and Evict

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated ReA ACS, radio

Documentation: Search-and-Evict Procedure for ReA6 Experimental Vault – Credited Administrative Control with ESH Impact

K500

Cyclotron Vault

Enterprise Competency: Perform a K500 Search-and-Evict

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated K500 ACS, portable O2 monitor (for the basement and sub-basement levels), radio

Documentation: Search-and-Evict Procedure for K500 Vault -- Credited Administrative Control with ESH Impact

User Vault (1500P/P1)

Enterprise Competency: Perform K500 User Vault Search-and-Evict

Staffing: Minimum of one (1) fully trained and authorized person

Equipment: Validated K500 ACS, radio

Documentation: Search-and-Evict Procedure for K500 User Vault Rm 1500P/P1 -- Credited Administrative Control with ESH Impact